|  |  |  |
| --- | --- | --- |
|  |  | Artisan X-e Deluxe |
|  |  | Energy Efficient Fluid BedCoffee Roasting System |

|  |
| --- |
| Artisan X-e Deluxe Complete Roasting & Bean Cooling System Specifications |
| Roaster Production | 50-60 lbs per hour |
| Roast Time | 8-12 minutes (manually adjustable) |
| Chaff Collection | Stand-alone chaff canister filter system |
| Bean Cooling | External 10 lb capacity |
| Roast Air Temperature | Variable manual control Fahrenheit or Celsius |
| Bean Temperature Thermometer | Included |
| Roaster Power | 60 amp, 240V single phase |
| Exhaust System Power | 11 amp, 230V 60 Hz single phase |
| Roaster Heat | 10400 watts |
| Batch Size | 2lb to 10lbs |
| Venting | Intake: 4” metal ducting (provided)Discharge: 5” metal ducting (not included) |
| Minimum Floor Space for full system | 7’ wide by 3’ deep |

|  |
| --- |
| Dimensions & Weight |
| Roaster/Exhaust Hood | 55” wide x 67.5” tall |
| Exhaust Blower 1550 CFM | 16.25” wide x 19” deep x 19.75” tall |
| Shipping Weight | 360 lbs |
| Shipping Dimensions | 1 Pallet (40x48x60) |

|  |
| --- |
| Electricity Usage |
| Full 10 lb load | 0.3 kWh per pound |
| 2 lb load | 0.6 kWh per pound |



|  |
| --- |
| Certification |
| UL |  |
| CE |  |
| NSF-4 |  |

Coffee Crafters

708 S Clearwater Loop, Suite 105, Post Falls, ID 83854

(509)228-6916 – sales@coffeecrafters.com

**\***Roaster comes complete with exhaust hood, bean thermometer, bean cooler and complete vent kit.